Programmer Command-line Interfaces Release Notes

# Release Notes for Programmer Command-Line Interfaces

## MPLAB® PM3 Device Programmer

Microchip Technology's device programmer is the MPLAB PM3. This may be controlled by the command-line interfaces Visual PROCMD or PM3CMD. Release notes for these command-line interfaces may be viewed by clicking the desired link below.

- Visual PROCMD
- PM3CMD

## PRO MATE™ II Device Programmer

PRO MATE II is an end-of-life product and has no new device support. Please consider using the MPLAB PM3.

A device programmer that is no longer in production but still supported, the PRO MATE II, may be controlled by the command-line interfaces Visual PROCMD or PROCMD. Release notes for these command-line interfaces may be viewed by clicking the desired link below.

- Visual PROCMD
- PROCMD

## MPLAB REAL ICE™ In-Circuit Emulator, MPLAB ICD 3 and PICkit 3 In-Circuit Debuggers

Microchip Technology's MPLAB REAL ICE In-Circuit Emulator may be controlled as a programmer by the command-line interface REALICECMD.
Microchip Technology's MPLAB ICD 3 In-Circuit Debugger may be controlled as a programmer by the command-line interface ICD3CMD.
Microchip Technology's PICkit 3 In-Circuit Debugger may be controlled as a programmer by the command-line interface PK3CMD.
Release notes for these command-line interfaces may be viewed by clicking the desired link below.

- REALICECMD and ICD3CMD
- Readme for PK3CMD.txt